**1494G 30 and 60 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 30 | 208 - 240 | 30 | H | 1494G-BC3H21494G-BF3H21494G-BK3H2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | J | 1494G-BC3J21494G-BF3J21494G-BK3J2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | R | 1494G-BC3R21494G-BF3R21494G-BK3R2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC302R |
| 30 | 480 - 600 | 30 | H | 1494G-BC3H61494G-BF3H61494G-BK3H6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | J | 1494G-BC3J61494G-BF3J61494G-BK3J6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | R | 1494G-BC3R61494G-BF3R61494G-BK3R6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30R |
| 60 | 208 - 240 | 60 | H | 1494G-CC3H21494G-CF3H21494G-CK3H2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | J | 1494G-CC3J21494G-CF3J21494G-CK3J2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | R | 1494G-CC3R21494G-CF3R21494G-CK3JR | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30R |
| 60 | 480 - 600 | 60 | H | 1494G-CC3H61494G-CF3H61494G-CK3H6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | J | 1494G-CC3J61494G-CF3J61494G-CK3J6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | R | 1494G-CC3R61494G-CF3R61494G-CK3R6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60R |

**1494G 100 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

Selecting Fuse Clips to Install a Larger or Smaller Fuse on 1494U Disconnect Switch. The fuse / fuse clip selection rules are listed below:

The 30 Amp 1494U-D30 Disconnect Switch and 1494U-F30 Trailer Fuse Block will accept 30 or 60 amp fuses.

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will accept 60 or 30 amp fuses.

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will not accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will not accept 200 Amp fuses.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 100 | 208 - 240 | 100 | H | 1494G-DC3H21494G-DJ3H21494G-DK3H2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | J | 1494G-DC3J21494G-DJ3J21494G-DK3J2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | R | 1494G-DC3R21494G-DJ3R21494G-DK3R2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |
| 100 | 480 - 600 | 100 | H | 1494G-DC3H61494G-DF3H61494G-DK3H6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | J | 1494G-DC3J61494G-DF3J61494G-DK3J6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | R | 1494G-DC3R61494G-DF3R61494G-DK3R6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

**1494GX 30 and 60 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 30 | 208 - 240 | 30 | H | 1494GX-BC3H21494GX-BF3H21494GX-BK3H2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | J | 1494GX-BC3J21494GX-BF3J21494GX-BK3J2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | R | 1494GX-BC3R21494GX-BF3R21494GX-BK3R2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC302R |
| 30 | 480 - 600 | 30 | H | 1494GX-BC3H61494GX-BF3H61494GX-BK3H6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | J | 1494GX-BC3J61494GX-BF3J61494GX-BK3J6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | R | 1494GX-BC3R61494GX-BF3R61494GX-BK3R6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30R |
| 60 | 208 - 240 | 60 | H | 1494GX-CC3H21494GX-CF3H21494GX-CK3H2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | J | 1494GX-CC3J21494GX-CF3J21494GX-CK3J2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | R | 1494GX-CC3R21494GX-CF3R21494GX-CK3JR | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30R |
| 60 | 480 - 600 | 60 | H | 1494GX-CC3H61494GX-CF3H61494GX-CK3H6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | J | 1494GX-CC3J61494GX-CF3J61494GX-CK3J6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | R | 1494GX-CC3R61494GX-CF3R61494GX-CK3R6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60R |

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

Selecting Fuse Clips to Install a Larger or Smaller Fuse on 1494U Disconnect Switch. The fuse / fuse clip selection rules are listed below:

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will accept 60 or 30 amp fuses.

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will not accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will not accept 200 Amp fuses.

**1494GX 100 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 100 | 208 - 240 | 100 | H | 1494GX-DC3H21494GX-DJ3H21494GX-DK3H2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | J | 1494GX-DC3J21494GX-DJ3J21494GX-DK3J2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | R | 1494GX-DC3R21494GX-DJ3R21494GX-DK3R2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |
| 100 | 480 - 600 | 100 | H | 1494GX-DC3H61494GX-DF3H61494GX-DK3H6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | J | 1494GX-DC3J61494GX-DF3J61494GX-DK3J6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | R | 1494GX-DC3R61494GX-DF3R61494GX-DK3R6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

**1494GY 30 and 60 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 30 | 208 - 240 | 30 | H | 1494GY-BC3H21494GY-BF3H21494GY-BK3H2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | J | 1494GY-BC3J21494GY-BF3J21494GY-BK3J2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 208 - 240 | 30 | R | 1494GY-BC3R21494GY-BF3R21494GY-BK3R2 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC302R |
| 30 | 480 - 600 | 30 | H | 1494GY-BC3H61494GY-BF3H61494GY-BK3H6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | J | 1494GY-BC3J61494GY-BF3J61494GY-BK3J6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30J |
| 30 | 480 - 600 | 30 | R | 1494GY-BC3R61494GY-BF3R61494GY-BK3R6 | 1494U-D30 | 1494U-F30 | 1494U-LA36 | 1494U-FC30R |
| 60 | 208 - 240 | 60 | H | 1494GY-CC3H21494GY-CF3H21494GY-CK3H2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | J | 1494GY-CC3J21494GY-CF3J21494GY-CK3J2 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30J |
| 60 | 208 - 240 | 60 | R | 1494GY-CC3R21494GY-CF3R21494GY-CK3JR | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC30R |
| 60 | 480 - 600 | 60 | H | 1494GY-CC3H61494GY-CF3H61494GY-CK3H6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | J | 1494GY-CC3J61494GY-CF3J61494GY-CK3J6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60J |
| 60 | 480 - 600 | 60 | R | 1494GY-CC3R61494GY-CF3R61494GY-CK3R6 | 1494U-D60 | 1494U-F60 | 1494U-LA36 | 1494U-FC60R |

|  |  |  |  |
| --- | --- | --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  Trailer Fuse Block (less phase barriers) |  |  |

**1494GY 100 Amp Disconnect Switch, Trailer Fuse Block and Fuse Clip Repair Parts**

Selecting Fuse Clips to Install a Larger or Smaller Fuse on 1494U Disconnect Switch. The fuse / fuse clip selection rules are listed below:

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will accept 60 or 30 amp fuses.

The 60 Amp 1494U-D60 Disconnect Switch and 1494U-F60 Trailer Fuse Block will not accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will accept 100 Amp fuses.

The 100 Amp 1494U-D100 Disconnect Switch and 1494U-F100 Trailer Fuse Block will not accept 200 Amp fuses.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Amps** | **Line Voltage** | **Fuse Clip Rating (A)** | **Fuse Clip Class** | **Catalog** **Number of Disconnect** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Trailer Fuse Block less Lugs, Fuse Clips and Phase Barriers** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** | **Fuse Clip Kit (includes 6 clips)** |
| 100 | 208 - 240 | 100 | H | 1494GY-DC3H21494GY-DJ3H21494GY-DK3H2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | J | 1494GY-DC3J21494GY-DJ3J21494GY-DK3J2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 208 - 240 | 100 | R | 1494GY-DC3R21494GY-DJ3R21494GY-DK3R2 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |
| 100 | 480 - 600 | 100 | H | 1494GY-DC3H61494GY-DF3H61494GY-DK3H6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | J | 1494GY-DC3J61494GY-DF3J61494GY-DK3J6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100J |
| 100 | 480 - 600 | 100 | R | 1494GY-DC3R61494GY-DF3R61494GY-DK3R6 | 1494U-D100 | 1494U-F100 | 1494U-LA100 | 1494U-FC100R |

# Phase Barriers, Protective Fuse Covers, Line Side Cover Fusible Disconnect Switches and/or Trailer Fuse Block Assemblies

One phase barrier catalog number contains 2 barriers; one for the disconnect switch, one for the trailer fuse block.

|  |  |  |
| --- | --- | --- |
| Phase Barriers for Disconnect Switch and Trailer Fuse Block | Protective Fuse Cover | Disconnect Switch Line Side Cover |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Amps** | **Catalog** **Number of Disconnect** **(starting with…)** | **Phase Barriers for Disconnect Switch and Trailer Fuse Block** | **Protective Fuse Cover** | **Disconnect Switch Line Side Cover** |
| 30, 60 | 1494G-B, 1494G-C, 1494GX-G, 1494GX-C, 1494GY-B, 1494GY-C | 1494U-PB31(Pkg Qty 2) | 1494U-PC1(30A - 60A, 250V Class H/R, 30A - 60A, 250V/600V Class J Fuses)or1494U-PC3(30A - 60A, 600V Class H/R, 100A, 250V/600V Class H/J/R Fuses) | 1494U-K31 |
| 100 | 1494G-D, 1494GX-D, 1494GY-D |

**Fuse Clip Kit Repair Parts (Class H, J fuse clips)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Fuse Clip Rating (A)** | **Fuse Clip Part No.** Contains six fuse clips and mounting hardware. | **Clamp Screw****(Item 1)** | **Clamp Block****(Item 3)** |
| 100 | 1494U-FC100J | 40023-110-02 | 40023-108-02 |

**Non-Fusible Disconnect Switch Repair Parts**

|  |  |
| --- | --- |
| Disconnect Switch With Mechanism, Line Side Cover and Three Line Side Lugs |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NEMA Size** | **Line Voltage** | **Catalog Number of Disconnect Switch** | **Disconnect Switch and Mechanism With Line Side Cover and Line Side Lugs** | **Lug Kit for Line or Load Side Lugs (1 kit contains 3 lugs)** |
| 30 | 208 | 1494G-BC3N, 1494G-BF3N | 1494U-D30 | 1494U-LA36 |
| 30 | 240 | 1494G-BC3N, 1494G-BF3N | 1494U-D30 | 1494U-LA36 |
| 30 | 480 | 1494G-BC3N, 1494G-BF3N | 1494U-D30 | 1494U-LA36 |
| 30 | 600 | 1494G-BC3N, 1494G-BF3N | 1494U-D30 | 1494U-LA36 |
| 60 | 208 | 1494G-CC3N, 1494G-CF3N | 1494U-D60 | 1494U-LA36 |
| 60 | 240 | 1494G-CC3N, 1494G-CF3N | 1494U-D60 | 1494U-LA36 |
| 60 | 480 | 1494G-CC3N, 1494G-CF3N | 1494U-D60 | 1494U-LA36 |
| 60 | 600 | 1494G-CC3N, 1494G-CF3N | 1494U-D60 | 1494U-LA36 |
| 100 | 208 | 1494G-DC3N, 1494G-DF3N | 1494U-D100 | 1494U-LA100 |
| 100 | 240 | 1494G-DC3N, 1494G-DF3N | 1494U-D100 | 1494U-LA100 |
| 100 | 480 | 1494G-DC3N, 1494G-DF3N | 1494U-D100 | 1494U-LA100 |
| 100 | 600 | 1494G-DC3N, 1494G-DF3N | 1494U-D100 | 1494U-LA100 |

**Handle and Mechanism Repair Parts**

Operating Handle part numbers include two bags of hardware which include the defeater lever, door cover catch, and handle gasket.

|  |  |
| --- | --- |
| Operating Handle with Studs (1494U-HP1 shown) | Connecting Rod Spring for Operating Handle |
| **Amps** | **Catalog** **Number of Disconnect** | **Enclosure NEMA Type** | **Operating Handle (with studs)** | **Connecting Rod and Spring Bracket** | **Spring for Operating Handle** |
| 30, 60 | 1494G-BF, 1494G-CF, 1494GX-BF, 1494GX-CF, 1494GY-BF, 1494GY-CF | 3R/4/12 | 1494U-HP1 | 1494U-R1 ➀ | Included with 1494U Operating Handle Part Numbers.  |
| 30, 60 | 1494G-BC, 1494G-CC, 1494GX-BC, 1494GX-CC, 1494GY-BC, 1494GY-CC | 4/4X(stainless steel) | 1494U-HS1 | 1494U-R1 ➀ | Included with 1494U Operating Handle Part Numbers.  |
| 100 | 1494G-DF, 1494GX-DF, 1494GY-DF | 3R/12 | 1494U-HP1 | 1494U-R1 ② | Included with 1494U Operating Handle Part Numbers. |
| 100 | 1494G-DC, 1494GX-DC, 1494GY-DC | 4/4X(stainless steel) | 1494U-HS1 | 1494U-R1 ② |

➀ Cut the Connecting Rod supplied with the 1494U-R1 Kit to an overall length of 4.40 inches

② Cut the Connecting Rod supplied with the 1494U-R1 Kit to an overall length of 5.0 inches

**Miscellaneous Repair Parts**

|  |  |  |  |
| --- | --- | --- | --- |
| **Description of Renewal Part** | **1494G-B, 1494GX-B, 1494GY-B 30 Amp Switches** | **1494G-C, 1494GX-C, 1494GY-C 60 Amp Switches** | **1494G-D, 1494GX-D, 1494GY-D 100 Amp Switches** |
| **Repair Part Number** | **Repair Part Number** | **Repair Part Number** |
| **Line Lug for Disconnect Switch and Load Lug for Trailer Fuse Block** | 1494U-LA36 ➀ | 1494U-LA36 ➀ | 1494U-LA100 ➀ |
| **Optional Copper Lug for Disconnect Switch and Load Lug for Trailer Fuse Block** | 1494U-LC36 ➀ | 1494U-LC36 ➀ | 1494U-LC100 ➀ |
| **Auxiliary Contact 1 N.O.** | 1494U-NO | 1494U-NO | 1494U-NO |
| **Auxiliary Contact 1 N.C.** | 1494U-NC | 1494U-NC | 1494U-NC |
| **Auxiliary Contact 1 N.O. Low Level** | 1494U-NOLV | 1494U-NOLV | 1494U-NOLV |
| **Auxiliary Contact 1 N.C. Low Level** | 1494U-NCLV | 1494U-NCLV | 1494U-NCLV |
| **Enclosure Conduit Hubs (used only on type 4/4X enclosures)** | (2) 1490-N10(1) 1490-N9 | (2) 1490-N10(1) 1490-N9 | (2) 1490-N5; (1) 1490-N9 |

➀ Part number contains 3 lugs.