|  |  |  |
| --- | --- | --- |
| **J1000 / S4 / S4 Plus** | | |
| **Part Number** | **Description** | **Availability** |
| ENM25335 | Cover, S4 Keyboard | A |
| A16196 | Ribbon cable – bottom of rack / motor control – IP65 only | I |
| A17362 | Circuit board rail (x10) | I |
| A13092 | S4 Plus upgrade kit (Lid, PC, Display, Ribbon Cable, Daughter board | I |
| ENM4479 | 90° white palstic elbow above ink and solvent tanks | I |
| ENM4839 | T fitting above ink and solvent tanks | A |
| ENM5044 | ELV Coaxial kit | A |
| ST6589 | Fan wiring harness | A |
| A12966 | RAM memory option | A |
| ENM4474 | Support (x5) Card H10 M4 MAL D4 | A |
| A21104 | 2MB SRAM card | O |
| EN6193 | Complete board rack | I |
| ST7206 | Rear cover for 4-jet head | A |
| ENM16208 | Governor (x10) – 0.3mm (id); 1.77mm (od) | A |
| ENM5044 | Electrovalve | A |
| ENM5675 | Canon Holder | A |

|  |  |  |
| --- | --- | --- |
| **SI / Contrast Specific** | | |
| **Part Number** | **Description** | **Availability** |
| ENM4262 | Accumulator O-ring | A |
| A13517 | Venturi | A |
| ENR19596 | Print Module – Contrast – Single jet – G – 5 meter | I |
| ST5258 | Recuperation gutter tube (SI) | O |

|  |  |  |
| --- | --- | --- |
| **S7** | | |
| **Part Number** | **Description** | **Availability** |
| ENM5366 | Duct hold – ink mod seal | A |
| A34679 | Service Suitcase User Kit (Canon Adj Screwdriver, 2x pin tools) | O |

|  |  |  |
| --- | --- | --- |
| **S7S** | | |
| **Part Number** | **Description** | **Availability** |
| A19233 | Handheld Terminal (A04) | A |

|  |  |  |
| --- | --- | --- |
| **Postal** | | |
| **Part Number** | **Description** | **Availability** |
| ENR18610 | Print module R6 180°, water base | I |

|  |  |  |
| --- | --- | --- |
| **9040** | | |
| **Part Number** | **Description** | **Availability** |
| ENM37764 | Protection keyboard | A |
| ENM36762 | Door latch Assy | A |
| ENM5044 | Electrovalve | A |
| ENM5675 | Canon Holder | A |

|  |  |  |
| --- | --- | --- |
| **S8** | | |
| **Part Number** | **Description** |  |
| A26968 | Disk-on-chip | A |
| A25604 | S8 Master lid kit | P |
| A14115 | V24 Upgrade kit (Ribbon cable and Daughter board) | O |
| A14066 | RS-232 Daughter board | A |
| ENM10163 | Rear handle | A |
| ENM14124 | Aluminum plate (safety level block) | O |
| ENM20192 | Cover – Main filter | A |
| A23913 | Torque Screw M5 (Main filter cover) | O |
| A20341 | Peltier Condenser Block | O |
| A16155 | Peltier Condenser Heatsink | O |
| ENM14252 | MAINS filter | A |
| ST7098 | Brass inertia wheel (secondary motor/vacuum pump assy) |  |
| A20362 | Cover – Back S8 |  |
| ENM4475 | 300mA Fuse (x10) |  |
| ENM25805 | Board – Adaption RS485/RS422 |  |
| ENM27192 | Head Pressurization Restriction 0.7 x 2.7 (x5) |  |
| ENM4348 | Screw CHC M2 x 4 (x20) |  |
| ENM5407 | Recuperation Gutter Tube |  |
| AC00033 | 120V Bulb (EN5900/EN5898 Alarm Lamps) |  |
| ENM5044 | Electrovalve |  |
| ENM5675 | Canon Holder |  |

|  |  |  |
| --- | --- | --- |
| **9020/9030** | | |
| **Part Number** | **Description** |  |
| ENM28572 | Cable Gland Plate (no holes) |  |
| ENM34702 | Conduit Bracket Plate |  |
| ENM34703 | Conduit Bracket Plate (IP65) |  |
| ENR36675 | CPU Board (9020) |  |
| ENR36676 | CPU Board (9030) |  |
| ENM35809 | Electrical Cable Kit |  |
| ENM28678 | Display Screen |  |
| ENM34044 | 4-valve solenoid block |  |
| ENM35470 | Recovery Solenoid Valve |  |
| ENM28629 | ADP Board |  |
| ENM28309 | Piezo Board |  |
| A35426 | Trolley |  |
| A35955 | Universal Printhead Mounting Plate |  |
| A36056 | Seal Kit |  |
| ENM34024 | 9020 CPU |  |
| ENM27781 | 9030 CPU |  |

|  |  |  |
| --- | --- | --- |
| **Universal Parts** | | |
| **Part Number** | **Description** |  |
| A23948 | 1L Bottle (Empty) |  |