{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["LED"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LED","index":0,"n_rows":45,"n_cols":52,"rows_kept":45,"cut":false,"hidden":false,"merged":[[29,2,29,16],[30,2,30,16],[5,1,5,6],[14,4,16,5],[23,6,23,7],[22,6,22,7],[21,6,21,7],[20,6,20,7],[19,6,19,7],[18,6,18,7],[17,6,17,7],[14,6,16,7],[23,4,23,5],[22,4,22,5],[21,4,21,5],[20,4,20,5],[19,4,19,5],[18,4,18,5],[17,4,17,5],[13,1,13,31],[9,1,9,6],[9,7,9,31],[8,7,8,17],[14,13,16,14],[14,15,14,22],[15,21,16,22],[11,3,11,28],[34,2,34,16],[29,18,30,31],[28,18,28,31],[27,18,27,31],[25,1,25,31],[14,1,16,3],[14,8,14,11],[15,10,16,11],[23,8,23,9],[22,8,22,9],[21,8,21,9],[20,8,20,9],[19,8,19,9],[18,8,18,9],[17,8,17,9],[23,10,23,11],[22,10,22,11],[21,10,21,11],[20,10,20,11],[19,10,19,11],[0,25,2,31],[3,24,3,31],[4,24,4,31],[0,7,0,24],[2,10,2,21],[8,1,8,6],[7,1,7,6],[6,1,6,6],[7,7,7,17],[6,7,6,17],[5,7,5,17],[3,9,3,22],[5,18,5,21],[6,18,6,21],[7,18,7,21],[8,18,8,21],[8,22,8,31],[7,22,7,31],[6,22,6,31],[5,22,5,31],[23,23,23,31],[22,23,22,31],[21,23,21,31],[20,23,20,31],[19,23,19,31],[18,23,18,31],[17,23,17,31],[14,23,16,31],[17,1,23,3],[38,1,38,31],[39,1,40,31],[41,1,41,31],[32,2,33,16],[31,2,31,16],[28,2,28,16],[27,2,27,16],[15,18,16,20],[15,15,16,17],[18,10,18,11],[17,10,17,11],[23,13,23,14],[22,13,22,14],[21,13,21,14],[20,13,20,14],[19,13,19,14],[18,13,18,14],[17,13,17,14],[15,8,16,9],[34,18,34,31],[33,18,33,31],[32,18,32,31],[31,18,31,31]]}
[null,null,null,null,null,null,null,"DUROSTRIP V5™ LED ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"800-827-3692\n816-318-8000 ext. 5000\n Fax: 816-318-8100"]
[]
[null,null,null,null,null,null,null,null,null,null,"STAND-ALONE LIGHTBAR"]
[null,null,null,null,null,null,null,null,null,"Order Form",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rom.orders@safefleet.net"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.romcorp.com"]
[null,"Today's Date:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P.O.#:"]
[null,"Cust. Name:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Job #:"]
[null,"Cust Contact:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cust Part #:"]
[null,"Phone:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Requested Ship Date: "]
[null,"Contact Email:"]
[]
[null,null,null,"To Order an Integrated DuroStripTM V5 - refer to Shutter Order Forms\nFM-8.2-22 Series III / FM-8.2-401 Series IV"]
[]
[null,"DUROSTRIP V5™ - Stand-Alone Lightbar "]
[null,"Part #",null,null,"Nominal Length",null,"Actual Length",null,"Total LENGTH based on Mounting",null,null,null,null,"Qty\n",null,"Mounting Option",null,null,null,null,null,null,null,"Customer\n Part #\n(optional)"]
[null,null,null,null,null,null,null,null,"VHB Mounting Tape",null,"Mounting Slots or Blocks",null,"R03916  Blue / White",null,null,"3M VHB\nDual Sided\nMounting\nTape",null,null,"Mounting\nSlots",null,null,"Adjustable Mounting Blocks"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Mounting Tape"]
[null,"R04786",null,null,"6\"",null,"6.54\"",null,"11.25\"",null,"12.75\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04692"]
[null,null,null,null,"12\"",null,"11.81\"",null,"16.50\"",null,"18.00\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04693"]
[null,null,null,null,"18\"",null,"18.35\"",null,"23.00\"",null,"24.50\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04694"]
[null,null,null,null,"24\"",null,23.62,null,"28.25\"",null,"29.75\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04695"]
[null,null,null,null,"30\"",null,"30.16\"",null,"35.00\"",null,"36.50\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04696"]
[null,null,null,null,"42\"",null,"41.94\"",null,"46.75\"",null,"48.25\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04697"]
[null,null,null,null,"60\"",null,"60.35\"",null,"65.00\"",null,"66.50\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R04698"]
[]
[null,"DUROSTRIP V5™  Lightbar Features"]
[]
[null,"w","White LED has 367 Lumens per foot",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","Vibration tested to MIL 810 rev A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"  "]
[null,"w","White LED draws 0.35 amps; @ 12.8 VDC approx. per 12\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","Salt Spray - 1,000 hour testing, no corrosion"]
[null,"w","Extreme Temp Certified operation between -40º F to 185º F",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","Integrated lower profile system is less intrusive and more out of harms way"]
[null,"w","Waterproof design - IP67 rating"]
[null,"w","Exceeds NFPA 1901 standard",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","Integrates with R•O•M Door Ajar Switch"]
[null,"w","Streamline optic lens and fixed lumen output across                  9VDC-16DVC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","Stand-alone light is available for interior or exterior"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w","7-year warranty"]
[null,"w","May be \"switched to positive\" or \"switched to negative\""]
[]
[]
[]
[null,"Comments"]
[]
[]
[null," Copyright 2024. R•O•M, a Safe Fleet Brand All Rights Reserved. Information contained is confidential & proprietary intellectual property of R•O•M."]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]